Dogpound p/n 60048
Assembly

1. Place one hotdog shelf on the lower 

level of steamer with short side in the middle. 
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2. Place second hotdog shelf on lower level 

of steamer next to other shelf with long side in 

middle.
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3. Place bun shelf on upper level support bolts 

as shown. 
[image: image3.jpg]



4. Place bun rack on bun shelf with the short

legs down for a condensation gap.
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5. Locate sliding glass door channels in front of 

steamer. Slide first door in rear channel, top first, 

with handles toward outer edge.  Repeat with second 

door in front sliding door channel.
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